Master Switch Three-Phase
MTS 100 3P
INPUT		
Voltage	380 / 400 / 415 V three-phase + N 	
Voltage tolerance	180 / 264 (selectable) 	
Frequency	50 / 60 Hz 	
Frequency tolerance	±10% (selectable)	
Switched input phases	3 (3-pole) 	
Distribution compatibility	IT, TT, TNS, TNC	
ENVIRONMENTAL		
Color	RAL 7024 	
Protection rating	IP20 	
Other compliances	 EN 62310-1 (safety) EN 62310-2 (electro-magnetic compatibility) 	
Noise (at 1 m)	55 dBA 	
Operating temperature	0 °C - +40 °C	
Storing temperature	-10 °C up to +50 °C	
Relative humidity	5-95% non-condensing	
Transport	Pallet jack  	
Available transfer modes	Automatic / Manual / Remote	
DATA		
Weight	150 kg	
Dimensions (h w d)	1500x685x530 mm