Multi Switch
MSW
INPUT		
Voltage	180-276 (selectable) 	
Frequency	50 / 60 Hz 	
Switched input phases	ph+N (two poles) 	
ENVIRONMENTAL		
Color	RAL 5004 	
Communication	RS232 / Slot for communication interface 	
Protection rating	IP20 	
Other compliances	EN 62310-1 (safety) EN 62310-2 (electro-magnetic compatibility) 	
Noise (at 1 m)	<35 dBA 	
Operating temperature	0 °C - +40 °C	
Storing temperature	-10 °C up to +50 °C	
Relative humidity	5-95% non-condensing	
Output sockets	8 IEC 320 10 A 	
DATA		
Weight	10 kg	
Dimensions (h w d)	2U x 19" x 360 mm