Multi Socket PDU
MDU
INPUT		
Voltage	184-276 (selectable) 	
Frequency	50 / 60 Hz 	
ENVIRONMENTAL		
Color	RAL 5004 	
Communication	RS232 / USB / Slot for communication interface 	
Protection rating	IP20 	
Protections	Overcurrent - overvoltage - undervoltage - protection against energy back-feed	
Noise (at 1 m)	<25 	
Operating temperature	0 °C - 40 °C	
Relative humidity	5-95% non-condensing	
Output sockets	8 IEC-320 C13 (10 A) 	
DATA		
Weight	5 kg	
Dimensions (h w d)	1U x 19” x 250 mm