Sentinel Tower
STW 5000
INPUT		
Rated power	5000 VA	
Voltage	220 / 230 / 240 V 	
Voltage tolerance	230 V ±20% 	
Frequency	50 / 60 Hz ±5 	
Power factor	>0.98	
Current distorsion	≤5% for single-phase input	
BY PASS		
Voltage tolerance	180 / 264 V (selectable in ECO Mode or SMART ACTIVE Mode) 	
Frequency tolerance	Selected frequency ±5% (selectable by user) 	
OUTPUT and INVERTER OUTPUT		
Rated power	5000 VA	
Active power	5000 W	
Rated voltage	220 / 230 / 240 V selectable 	
Crest factor (Ipeak/Irms)	3 : 1 	
Waveform	Sinusoidal 	
Frequency	50 / 60 Hz selectable 	
Voltage distortion with non-linear load	<3% 	
Voltage distortion with linear load	<1% 	
BATTERIES		
Type	VRLA AGM maintenance-free lead based 	
Typical recharge time	4-6 h 	
ENVIRONMENTAL		
Color	Black RAL 9005 	
Communication	USB / RS232 / slot for communications interface / REPO + Input contact 	
Accessories provided	USB cable 	
Surge capability	1 VDR x 300 J 	
Protections	Overcurrent - short circuit - overvoltage - undervoltage - temperature - excessive low battery	
Noise (at 1 m)	<48 [bBA] (ECO Mode) 	
Operating temperature	0 °C - +40 °C	
Relative humidity	5-95% non-condensing	
Output sockets	Terminal block + 2 IEC 320 C13 	
Standards	European directives: L V 2014/35/EU low voltage; EMC 2014/30/EU electromagnetic compatibility -- Directive and Standards: Safety IEC EN 62040-1; EMC IEC EN 62040-2; RoHS compliant -- Classification in accordance with IEC 62040-3 VFI - SS - 111 	
DATA		
Weight	62 kg	
Dimensions (h w d)	250x698x500 mm